**Wifi Pineapple: Evil Portal**

Plug the Wifi Pineapple into your device or power source

Open a web browser and navigate to 172.16.42.1:1471

Login to the Wifi Pineapple

On the left hand side of the screen there is a taskbar. Select the sixth option that looks like a puzzle piece to bring up the Modules & Packages tab.

Graphical user interface, application

Description automatically generated

Navigate to the Available Modules tab at the top of the screen and click the button labelled “Get Available Modules”.

Graphical user interface, application, Teams

Description automatically generated

Select the Evil Portal module and install it to the Wifi Pineapple. Then navigate to the Installed Modules tab at the top of the screen.

Graphical user interface, text, application

Description automatically generated

Click on the Evil Portal box to bring up the Evil Portal tab.

A screenshot of a computer

Description automatically generated with medium confidence

You can either create a new portal or add a portal to the Portal Library using a USB. (Instructions on how to add portals using a USB are added at the end of these instructions)

Text


Description automatically generated

Once a portal is added, in the Portal Library tab you can see the list of portal names. You can download, preview, or view log of each portal. To enable the portal, select the Activate option.

Graphical user interface, website

Description automatically generated

Then make sure that Start and Start Web Server is selected at the top of the screen.



Now when devices connect to the Wifi Pineapple’s access point, it should bring up a login page.

Graphical user interface, application

Description automatically generated


You can see the login information by viewing the log for the portal.


Text, letter

Description automatically generated


**How to add the evil portal templates from a USB device**

Go to the Wifi Pineapple Evil Portal Templates folder on the Google drive and copy the evilportals-master folder onto a USB device. Insert the USB device into the Wifi Pineapple. Log into the Wifi Pineapple and click on the terminal icon at the top right corner of the screen next to the icon of the three vertical dots.





Navigate to the USB file location and copy the contents of the evilportals-master folder using the following command:



Now the portal templates should be displayed in the Evil Portal tab on the Wifi Pineapple.

